1
 
 
 
 
                   THIS PROGRAM IS CONFIDENTIAL AND A TRADE SECRET OF THE MACNEAL-SCHWENDLER CORP.  THE RECEIPT OR   
                  POSSESSION OF THIS PROGRAM DOES NOT CONVEY ANY RIGHTS TO REPRODUCE OR DISCLOSE ITS CONTENTS, OR TO 
                 MANUFACTURE, USE, OR SELL ANYTHING HEREIN, IN WHOLE OR IN PART, WITHOUT THE SPECIFIC WRITTEN CONSENT
                                               OF THE MACNEAL-SCHWENDLER CORPORATION.                                
 
 
                                              * * * * * * * * * * * * * * * * * * * *
                                              * * * * * * * * * * * * * * * * * * * *
                                              * *                                 * *
                                              * *               THE               * *
                                              * *        MACNEAL-SCHWENDLER       * *
                                              * *           CORPORATION           * *
                                              * *                                 * *
                                              * *      M S C / N A S T R A N      * *
                                              * *                                 * *
                                              * *        VERSION - 69.1.0         * *
                                              * *                                 * *
                                              * *          JAN 23, 1997           * *
                                              * *                                 * *
                                              * *                                 * *
                                              * *      IBM RISC System/6000       * *
                                              * *                                 * *
                                              * *    MODEL 370/37T/375 (fiji)     * *
                                              * *                                 * *
                                              * *             AIX 4.1             * *
                                              * *                                 * *
                                              * *                                 * *
                                              * *                                 * *
                                              * * * * * * * * * * * * * * * * * * * *
                                              * * * * * * * * * * * * * * * * * * * *
1 
                     Welcome to MSC/NASTRAN Version 69.1
  
    MSC/NASTRAN Version 69.1 is the latest release of MSC/NASTRAN.  It offers
    the following features and enhancements to extend the power and performance
    of MSC/NASTRAN Version 69.
  
    * Performance Improvements
      * Refinements to the performance, diagnostics, and shift logic of
        the SOLVIT, CEAD, and REIGL numerical processing modules.
      * Significant speed improvements for inertia relief analysis.
      * Performance improvements for the solution of frequency response
        problems.
  
    * Functionality Improvements
      * Acoustic symmetrization now available in modal frequency response.
      * The ability to define external superelements as "tip superelements"
        based on the partitioning methodology introduced in Version 69.
  
    * Quality and Reliability
      * The shell-solid connector element (RSSCON) now satisfies the rigid body
        requirements by automatically aligning its grid points within a
        user-modifiable tolerance.
  
      * Over 50 error corrections, which include corrections to defects in
        dynamics solution sequences and mini-databases.
  
    With MSC/NASTRAN Version 69.1, you benefit from all the rich functionality
    provided in Version 69. Version 69 offers you significant performance
    improvements, new capabilities, over 100 user driven enhancements, and over
    300 error corrections.
  
    MSC/NASTRAN Version 69 adds the following major new capabilities
    compared to Version 68.2:
  
    * Functionality Improvements
      * Shell-to-solid connector elements.
      * Beam cross-section library.
      * Corner stresses for hyperelastic elements.
  
      * Extensive Superelement enhancements
        * Duplicate grid and element IDs in Superelements.
        * Automatic attachment of superelements based on geometry.
        * Simplified superelement tree definition.
      * Dynamics Improvements
        * Frequency-dependent elements for dynamic analysis.
        * Acoustic analysis enhancements.
        * Adaptive excitation frequencies.
        * Logarithmic table input.
      * Optimization Improvements
1       * Mode tracking for design optimization.
        * New optimization print options and diagnostics.
        * Beam library Optimization.
  
    * Performance Improvements
      * The memory reduction of Version 69 enables you to run larger models and
        may quadruple the throughput of MSC/NASTRAN on your server or
        supercomputer.
      * New iterative solver features.
      * 64-bit data representation.
      * Mini-database restarts.
      * Faster statics, normal modes, and dynamics analyses.
        * More efficient sparse solver and Lanczos eigenvalue extraction method.
        * More efficient acoustic and frequency response solution methods.
  
    * Ease of use Improvements
      * A new resource estimator.
      * Enhanced NASTRAN statement.
  
    The following changes were made in Version 69 relative to Version 68 based
    systems:
  
      * The database is not compatible with Version 68
      * The sequencer is turned off by default.
      * The unstructured solution sequences (SOL 60-99) are no longer available.
  
    For complete descriptions of all V69 and V69.1 enhancements, please refer to
    the MSC/NASTRAN Release Guides for these versions.
  
    This "news" information can be turned off by changing news=yes to
    news=no in the system runtime configuration (rc) file. Once turned
    off in the system rc file, it can be turned on by setting news=yes
    in the MSC/NASTRAN command line or local rc file.
1                                                                               MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     1
                                                                                                                                    
0        N A S T R A N    F I L E    A N D    S Y S T E M    P A R A M E T E R    E C H O                                           
0                                                                                                                                   
                                                                                                                                    
                                                                                                                                    
     NASTRAN BUFFSIZE=12801                                                          
1                                                                               MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     2
                                                                                                                                    
0        N A S T R A N    E X E C U T I V E    C O N T R O L    D E C K    E C H O                                                  
0                                                                                                                                   
                                                                                                                                    
                                                                                                                                    
     ID     LINEAR,INERTIA2                                                          
     SOL    101                                                                              
     TIME   5                                                                                
     CEND                                                                                    
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     3
                                                                                                                                    
0                                                                                                                                   
0                                        C A S E    C O N T R O L   D E C K   E C H O                                               
                 CARD                                                                                                               
                 COUNT                                                                                                              
                  1      TITLE = BAR WITH SUPORT ENTRY                                                           
                  2      LOAD = 1                                                                                
                  3      DISP = ALL                                                                              
                  4      SPCF = ALL                                                                              
                  5      STRESS = ALL                                                                            
                  6      BEGIN BULK                                                                              
0                             INPUT BULK DATA CARD COUNT =      32
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     4
                                                                                                                                    
0                                                                                                                                   
0                                                 S O R T E D   B U L K   D A T A   E C H O                                         
                 CARD                                                                                                               
                 COUNT        .   1  ..   2  ..   3  ..   4  ..   5  ..   6  ..   7  ..   8  ..   9  ..  10  .                      
                    1-        CBEAM   1       1       1       2       1.      1.      0.0                     
                    2-        CBEAM   2       1       2       3       1.      1.      0.0                     
                    3-        CBEAM   3       1       3       4       1.      1.      0.0                     
                    4-        GRID    1               0.0     0.0     0.0                                     
                    5-        GRID    2               10.     0.0     0.0                                     
                    6-        GRID    3               20.     0.0     0.0                                     
                    7-        GRID    4               30.     0.0     0.0                                     
                    8-        MAT1    1       1.+7            .3      7.43E-3                                 
                    9-        PARAM   GRDPNT  3                                                               
                   10-        PARAM   INREL   -1                                                              
                   11-        PARAM   POST    -1                                                              
                   12-        PBEAM   1       1       1.      .667    .167            .1               +000001
                   13-        ++000001.1      .1      .1      -.1     -.1     .1      -.1     -.1      +000002
                   14-        PLOAD1  1       1       FY      FR      0.      1000.   1.      1000.           
                   15-        PLOAD1  1       2       FY      FR      0.      1000.   1.      1000.           
                   16-        PLOAD1  1       3       FY      FR      0.      1000.   1.      1000.           
                   17-        SUPORT  3       123456                                                          
                              ENDDATA 
0                       TOTAL COUNT=        18
0*** USER INFORMATION MESSAGE 4109 (OUTPX2)  THE LABEL IS XXXXXXXX FOR FORTRAN UNIT 12
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =        7 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =        8 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR TAPE LABEL =       17 WORDS.)
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK GEOM1S   WRITTEN ON FORTRAN UNIT 12, TRL = 
                101                 0                 0                 8                 0                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =       35 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =       66 WORDS.)
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK GEOM2S   WRITTEN ON FORTRAN UNIT 12, TRL = 
                102                 0                 0                 0              1024                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =       57 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =       88 WORDS.)
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK GEOM3S   WRITTEN ON FORTRAN UNIT 12, TRL = 
                103                 0                 0                 0                 0              2048                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =       27 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =       58 WORDS.)
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     5
                                                                                                                                    
0                                                                                                                                   
0                                                                                                                                   
                                                                                                                                    
                                                                                                                                    
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK GEOM4S   WRITTEN ON FORTRAN UNIT 12, TRL = 
                104                 0                 0                 0               256                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =        7 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =       36 WORDS.)
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK EPTS     WRITTEN ON FORTRAN UNIT 12, TRL = 
                105                 0                 0                 0              1024                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =      200 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =      231 WORDS.)
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK MPTS     WRITTEN ON FORTRAN UNIT 12, TRL = 
                101             32768                 0                 0                 0                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =       15 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =       46 WORDS.)
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     6
                                                                                                                                    
0                                                                                                                                   
                           O U T P U T   F R O M   G R I D   P O I N T   W E I G H T   G E N E R A T O R
0                                                     REFERENCE POINT =        3
                                                                M O
                      *  2.229000E-01  0.000000E+00  0.000000E+00  0.000000E+00  0.000000E+00  0.000000E+00 *
                      *  0.000000E+00  2.229000E-01  0.000000E+00  0.000000E+00  0.000000E+00 -1.114500E+00 *
                      *  0.000000E+00  0.000000E+00  2.229000E-01  0.000000E+00  1.114500E+00  0.000000E+00 *
                      *  0.000000E+00  0.000000E+00  0.000000E+00  1.858986E-01  0.000000E+00  0.000000E+00 *
                      *  0.000000E+00  0.000000E+00  1.114500E+00  0.000000E+00  2.600500E+01  0.000000E+00 *
                      *  0.000000E+00 -1.114500E+00  0.000000E+00  0.000000E+00  0.000000E+00  2.600500E+01 *
                                                                 S
                                           *  1.000000E+00  0.000000E+00  0.000000E+00 *
                                           *  0.000000E+00  1.000000E+00  0.000000E+00 *
                                           *  0.000000E+00  0.000000E+00  1.000000E+00 *
                               DIRECTION
                          MASS AXIS SYSTEM (S)     MASS              X-C.G.        Y-C.G.        Z-C.G.
                                  X            2.229000E-01      0.000000E+00  0.000000E+00  0.000000E+00
                                  Y            2.229000E-01     -5.000000E+00  0.000000E+00  0.000000E+00
                                  Z            2.229000E-01     -5.000000E+00  0.000000E+00  0.000000E+00
                                                                I(S)
                                           *  1.858986E-01  0.000000E+00  0.000000E+00 *
                                           *  0.000000E+00  2.043250E+01  0.000000E+00 *
                                           *  0.000000E+00  0.000000E+00  2.043250E+01 *
                                                                I(Q)
                                           *  1.858986E-01                             *
                                           *                2.043250E+01               *
                                           *                              2.043250E+01 *
                                                                 Q
                                           *  1.000000E+00  0.000000E+00  0.000000E+00 *
                                           *  0.000000E+00  1.000000E+00  0.000000E+00 *
                                           *  0.000000E+00  0.000000E+00  1.000000E+00 *

1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     7
                                                                                                                                    
0                                                                                                                                   
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     8
                                                                                                                                    
0                                                                                                                                   
0 RESULTANTS ABOUT        3 IN SUPERELEMENT BASIC SYSTEM COORDINATES.

0                                                  OLOAD    RESULTANT       
0                 T1             T2             T3             R1             R2             R3
0        1   0.0000000E+00  3.0000000E+04  0.0000000E+00  0.0000000E+00  0.0000000E+00 -1.5000000E+05
0        2  -2.2290000E-01  0.0000000E+00  0.0000000E+00  0.0000000E+00  0.0000000E+00  0.0000000E+00
0        3   0.0000000E+00 -2.2290000E-01  0.0000000E+00  0.0000000E+00  0.0000000E+00  1.1145000E+00
0        4   0.0000000E+00  0.0000000E+00 -2.2290000E-01  0.0000000E+00 -1.1145000E+00  0.0000000E+00
0        5   0.0000000E+00  0.0000000E+00  0.0000000E+00 -1.8589860E-01  0.0000000E+00  0.0000000E+00
0        6   0.0000000E+00  0.0000000E+00 -1.1145000E+00  0.0000000E+00 -2.6005001E+01  0.0000000E+00
0        7   0.0000000E+00  1.1145000E+00  0.0000000E+00  0.0000000E+00  0.0000000E+00 -2.6005001E+01
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE     9
                                                                                                                                    
0                                                                                                                                   
0*** USER INFORMATION MESSAGE 3035 FOR DATA BLOCK   KLR     

    SUPPORT PT.NO.             EPSILON             STRAIN   ENERGY     EPSILONS LARGER THAN  .001 ARE FLAGGED WITH ASTERISKS
                1          6.5731964E-16          0.0000000E+00                 
                2          6.5731964E-16          0.0000000E+00                 
                3          6.5731964E-16          0.0000000E+00                 
                4          6.5731964E-16          0.0000000E+00                 
                5          6.5731964E-16         -1.1641532E-10                 
                6          6.5731964E-16          2.3283064E-09                 
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    10
                                                                                                                                    
0                                                                                                                                   
                                                  INTERMEDIATE MATRIX ... QRR     


                                                            COLUMN      1
     1         2.229000E-01       0.000000E+00       0.000000E+00       0.000000E+00       0.000000E+00       0.000000E+00        6

                                                            COLUMN      2
     1         0.000000E+00       2.229000E-01       0.000000E+00       0.000000E+00       0.000000E+00      -1.114500E+00        6

                                                            COLUMN      3
     1         0.000000E+00       0.000000E+00       2.229000E-01       0.000000E+00       1.114500E+00       0.000000E+00        6

                                                            COLUMN      4
     1         0.000000E+00       0.000000E+00       0.000000E+00       1.858986E-01       0.000000E+00       0.000000E+00        6

                                                            COLUMN      5
     1         0.000000E+00       0.000000E+00       1.114500E+00       0.000000E+00       2.600500E+01       0.000000E+00        6

                                                            COLUMN      6
     1         0.000000E+00      -1.114500E+00       0.000000E+00       0.000000E+00       0.000000E+00       2.600500E+01        6

1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    11
                                                                                                                                    
0                                                                                                                                   
                                                  INTERMEDIATE MATRIX ... QRL     


                                                            COLUMN      1
     1         0.000000E+00      -3.000000E+04       0.000000E+00       0.000000E+00       0.000000E+00       1.500000E+05        6

1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    12
                                                                                                                                    
0                                                                                                                                   
                                                  INTERMEDIATE MATRIX ... URA     


                                                            COLUMN      1
     1         0.000000E+00       1.345895E+05       0.000000E+00       0.000000E+00       0.000000E+00       1.416458E-12        6

0*** USER INFORMATION MESSAGE 5293 FOR DATA BLOCK KLL     

    LOAD SEQ. NO.             EPSILON              EXTERNAL WORK      EPSILONS LARGER THAN  .001 ARE FLAGGED WITH ASTERISKS
                1         -2.1134298E-15          1.5617191E+02
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    13
                                                                                                                                    
0                                                                                                                                   
0 RESULTANTS ABOUT        3 IN SUPERELEMENT BASIC SYSTEM COORDINATES.

0                                                  SPCFORCE RESULTANT       
0                 T1             T2             T3             R1             R2             R3
0        1   0.0000000E+00  4.1225057E-12  0.0000000E+00  0.0000000E+00  0.0000000E+00 -3.5533365E-27
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    14
                                                                                                                                    
0                                                                                                                                   
0                                                                                                                                   
                                                                                                                                    
                                                                                                                                    
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK OQG1     WRITTEN ON FORTRAN UNIT 12, TRL = 
                101                 0                32                 0                 0                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =      146 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =      211 WORDS.)
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK OUGV1    WRITTEN ON FORTRAN UNIT 12, TRL = 
                101                 0                32                 0                 0                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =      146 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =      211 WORDS.)
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    15
                                                                                                                                    
0                                                                                                                                   
 
                                             D I S P L A C E M E N T   V E C T O R
 
      POINT ID.   TYPE          T1             T2             T3             R1             R2             R3
             1      G       .0           -2.498751E-01    .0             .0             .0            2.498751E-02
             2      G       .0           -6.246877E-02    .0             .0             .0            1.249375E-02
             3      G       .0             .0             .0             .0             .0             .0
             4      G       .0           -6.246876E-02    .0             .0             .0           -1.249375E-02
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    16
                                                                                                                                    
0                                                                                                                                   
 
                               F O R C E S   O F   S I N G L E - P O I N T   C O N S T R A I N T
 
      POINT ID.   TYPE          T1             T2             T3             R1             R2             R3
             3      G       .0            4.122506E-12    .0             .0             .0           -3.553337E-27
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    17
                                                                                                                                    
0                                                                                                                                   
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    18
                                                                                                                                    
0                                                                                                                                   
 
                                  S T R E S S E S   I N   B E A M   E L E M E N T S        ( C B E A M )
                    STAT DIST/
   ELEMENT-ID  GRID   LENGTH    SXC           SXD           SXE           SXF           S-MAX         S-MIN         M.S.-T   M.S.-C
0         1
                  1    .000     .0            .0            .0            .0            .0            .0                   
                  2   1.000     .0            .0            .0            .0            .0            .0                   
0         2
                  2    .000     .0            .0            .0            .0            .0            .0                   
                  3   1.000     .0            .0            .0            .0            .0            .0                   
0         3
                  3    .000     .0            .0            .0            .0            .0            .0                   
                  4   1.000     .0            .0            .0            .0            .0            .0                   
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    19
                                                                                                                                    
0                                                                                                                                   
0*** USER INFORMATION MESSAGE 4114 (OUTPX2)
     DATA BLOCK OES1X    WRITTEN ON FORTRAN UNIT 12, TRL = 
                101                 0                 1                 1                 0                 0                 0
                                    (MAXIMUM POSSIBLE FORTRAN RECORD SIZE =    25602 WORDS.)
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =      333 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =       20 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR DATA BLOCK =      507 WORDS.)
0*** USER INFORMATION MESSAGE 4110 (OUTPX2)END-OF-DATA SIMULATION ON FORTRAN UNIT 12
                                 (MAXIMUM SIZE OF FORTRAN RECORDS WRITTEN =      1 WORDS.)
                                       (NUMBER OF FORTRAN RECORDS WRITTEN =      1 RECORDS.)
                                       (TOTAL DATA WRITTEN FOR EOF MARKER =      1 WORDS.)
1    BAR WITH SUPORT ENTRY                                                      MAY  20, 1997  MSC/NASTRAN   1/23/97   PAGE    20
                                                                                                                                    
0                                                                                                                                   
 * * * *  D B D I C T   P R I N T  * * * *      SUBDMAP = PRTSUM  ,  DMAP STATEMENT NO.     13



0                                   * * * *  A N A L Y S I S  S U M M A R Y  T A B L E  * * * *
0 SEID  PEID PROJ VERS APRCH      SEMG SEMR SEKR SELG SELR MODES DYNRED SOLLIN PVALID SOLNL LOOPID DESIGN CYCLE SENSITIVITY
 --------------------------------------------------------------------------------------------------------------------------
     0     0    1    1 '        '    T    T    T    T    T     F      F      T      0     F     -1            0           F
0SEID = SUPERELEMENT ID.
 PEID = PRIMARY SUPERELEMENT ID OF IMAGE SUPERELEMENT.
 PROJ = PROJECT ID NUMBER.
 VERS = VERSION ID.
 APRCH = BLANK FOR STRUCTURAL ANALYSIS.  HEAT FOR HEAT TRANSFER ANALYSIS.
 SEMG = STIFFNESS AND MASS MATRIX GENERATION STEP.
 SEMR = MASS MATRIX REDUCTION STEP (INCLUDES EIGENVALUE SOLUTION FOR MODES).
 SEKR = STIFFNESS MATRIX REDUCTION STEP.
 SELG = LOAD MATRIX GENERATION STEP.
 SELR = LOAD MATRIX REDUCTION STEP. 
 MODES = T (TRUE) IF NORMAL MODES OR BUCKLING MODES CALCULATED.
 DYNRED = T (TRUE) MEANS GENERALIZED DYNAMIC AND/OR COMPONENT MODE REDUCTION PERFORMED.
 SOLLIN = T (TRUE) IF LINEAR SOLUTION EXISTS IN DATABASE.
 PVALID = P-DISTRIBUTION ID OF P-VALUE FOR P-ELEMENTS
 LOOPID = THE LAST LOOPID VALUE USED IN THE NONLINEAR ANALYSIS.  USEFUL FOR RESTARTS.
 SOLNL = T (TRUE) IF NONLINEAR SOLUTION EXISTS IN DATABASE.
 DESIGN CYCLE = THE LAST DESIGN CYCLE (ONLY VALID IN OPTIMIZATION).
 SENSITIVITY = SENSITIVITY MATRIX GENERATION FLAG.
1                                        * * * END OF JOB * * *
 
 
