*Heading
** Job name: robust Model name: Model-1
** Generated by: Abaqus/CAE 6.9-1
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=wuerfel
*End Part
**  
**
** ASSEMBLY
**
*Assembly, name=Assembly
**  
*Instance, name=wuerfel-1, part=wuerfel
*Node
      1,         -25.,         -75.,         100.
      2,         -25.,         -25.,         100.
      3,         -25.,          25.,         100.
      4,         -25.,         -75.,          50.
      5,         -25.,         -25.,          50.
      6,         -25.,          25.,          50.
      7,         -25.,         -75.,           0.
      8,         -25.,         -25.,           0.
      9,         -25.,          25.,           0.
     10,          25.,         -75.,         100.
     11,          25.,         -25.,         100.
     12,          25.,          25.,         100.
     13,          25.,         -75.,          50.
     14,          25.,         -25.,          50.
     15,          25.,          25.,          50.
     16,          25.,         -75.,           0.
     17,          25.,         -25.,           0.
     18,          25.,          25.,           0.
     19,          75.,         -75.,         100.
     20,          75.,         -25.,         100.
     21,          75.,          25.,         100.
     22,          75.,         -75.,          50.
     23,          75.,         -25.,          50.
     24,          75.,          25.,          50.
     25,          75.,         -75.,           0.
     26,          75.,         -25.,           0.
     27,          75.,          25.,           0.
*Element, type=C3D8H
1, 10, 11, 14, 13,  1,  2,  5,  4
2, 11, 12, 15, 14,  2,  3,  6,  5
3, 13, 14, 17, 16,  4,  5,  8,  7
4, 14, 15, 18, 17,  5,  6,  9,  8
5, 19, 20, 23, 22, 10, 11, 14, 13
6, 20, 21, 24, 23, 11, 12, 15, 14
7, 22, 23, 26, 25, 13, 14, 17, 16
8, 23, 24, 27, 26, 14, 15, 18, 17
*Nset, nset=_PickedSet2, internal, generate
  1,  27,   1
*Elset, elset=_PickedSet2, internal, generate
 1,  8,  1
** Section: rubbersection
*Solid Section, elset=_PickedSet2, material=elastomer
,
*End Instance
**  
*Nset, nset=_PickedSet4, internal, instance=wuerfel-1, generate
  3,  27,   3
*Elset, elset=_PickedSet4, internal, instance=wuerfel-1, generate
 2,  8,  2
*Nset, nset=_PickedSet5, internal, instance=wuerfel-1, generate
 19,  27,   1
*Elset, elset=_PickedSet5, internal, instance=wuerfel-1, generate
 5,  8,  1
*Nset, nset=_PickedSet6, internal, instance=wuerfel-1
  1,  2,  3, 10, 11, 12, 19, 20, 21
*Elset, elset=_PickedSet6, internal, instance=wuerfel-1
 1, 2, 5, 6
*Nset, nset=_PickedSet7, internal, instance=wuerfel-1, generate
  1,  25,   3
*Elset, elset=_PickedSet7, internal, instance=wuerfel-1, generate
 1,  7,  2
*End Assembly
** 
** MATERIALS
** 
*Parameter
 C10 = 1
 C01=  0.2
*Material, name=elastomer
*Hyperelastic, n=2
 <C10>,<C01>,0.,0.,0.,0.,0.
** ----------------------------------------------------------------
** 
** STEP: belastung
** 
*Step, name=belastung, nlgeom=YES
*Static
0.1, 1., 1e-05, 0.1
** 
** BOUNDARY CONDITIONS
** 
** Name: BC-1 Type: Displacement/Rotation
*Boundary
_PickedSet4, 2, 2, 100.
** Name: BC-2 Type: Displacement/Rotation
*Boundary
_PickedSet5, 1, 1
** Name: BC-3 Type: Displacement/Rotation
*Boundary
_PickedSet6, 3, 3
** Name: BC-4 Type: Displacement/Rotation
*Boundary
_PickedSet7, 2, 2
** 
** OUTPUT REQUESTS
** 
*Restart, write, frequency=0
** 
** FIELD OUTPUT: F-Output-1
** 
*Output, field, variable=PRESELECT
** 
** HISTORY OUTPUT: H-Output-1
** 
*Output, history, variable=PRESELECT
*End Step
