/COM,ANSYS RELEASE 12.0.1  UP20090415       20:38:41    11/02/2010

 *** WARNING ***                         CP =       0.906   TIME= 20:38:48
 Element 1 is of type SOLID186, which is not a shell.  Such elements are 
 ignored by the shell-to-solid option of the CBDOF command.              

 *** WARNING ***                         CP =       0.906   TIME= 20:38:48
 No interpolation nodes lie on or near the selected elements.  The CBDO  
 operation produced no results.                                          

 *** WARNING ***                         CP =       0.922   TIME= 20:38:48
 /INPUT file does not contain line :CB1.                                 

 *** WARNING ***                         CP =       0.938   TIME= 20:38:48
 Element shape checking is currently inactive.  Issue SHPP,ON or         
 SHPP,WARN to reactivate, if desired.                                    

 *** WARNING ***                         CP =       1.203   TIME= 20:38:49
 Material number 3 (used by element 1561 ) should normally have at least 
 one MP or one TB type command associated with it.  Output of energy by  
 material may not be available.                                          

 *** WARNING ***                         CP =       3.109   TIME= 20:38:51
 Coefficient ratio exceeds 1.0e8 - Check results.                        
